|  |  |  |
| --- | --- | --- |
| * Basswood body
* Bolt-on hardrock Maple neck
* Burns original headstock
* Classic polyester finish
* Rosewood fingerboard
* Scale Length 25.5"
* Nut Width 49mm
* Truss rod Bi-flex two way type
* 21 frets
* Chrome hardware as standard
* Burns® de-luxe machine heads
* 3 x Burns® Tri-Sonic® pickups
* Five-way pickup switch
* Push/pull pickup selector
* One master volume
* Two-tone controls
* Rez-o-Tube® tremolo system

|  |
| --- |
| http://www.burnsguitars.com/images/gearomatic.jpg**Burns® Gear-o-Matik™ Gearbox**This Burns gearbox was first designed by Jim Burns in 1960 to allow fine neck setting. Coupled to the steel truss rod tensioned through the neck to a gearbox with a hefty cog and worm which provides micro adjustment. |

 |  |