|  |  |  |
| --- | --- | --- |
| * Basswood body * Bolt-on hardrock Maple neck * Burns original headstock * Classic polyester finish * Rosewood fingerboard * Scale Length 25.5" * Nut Width 49mm * Truss rod Bi-flex two way type * 21 frets * Chrome hardware as standard * Burns® de-luxe machine heads * 3 x Burns® Tri-Sonic® pickups * Five-way pickup switch * Push/pull pickup selector * One master volume * Two-tone controls * Rez-o-Tube® tremolo system  |  | | --- | | http://www.burnsguitars.com/images/gearomatic.jpg**Burns® Gear-o-Matik™ Gearbox** This Burns gearbox was first designed by Jim Burns in 1960 to allow fine neck setting. Coupled to the steel truss rod tensioned through the neck to a gearbox with a hefty cog and worm which provides micro adjustment. | |  |