**Year:** [1989](https://reverb.com/uk/marketplace/electric-guitars?year_max=1989&year_min=1989)

**Made In:** Japan

Maple neck in basswood body, maple fingerboard, 24 frets specification, 648 mm long scale, RMX - II lock type tremolo, original pickup mounted in S - S - H layout!
You can make it possible to create a wide range of sound with a simple control for bi-sound switch.